% DAR_#1.tex (example)
% Requires: \input{dar.tex} has been run once in main.tex

\renewcommand{\Aone}{u-blox MIA-M10C}
\renewcommand{\Atwo}{u-blox MAX-M10S}
\renewcommand{\Atri}{Quectel L86}

\renewcommand{\critA}{Energy pr. fix}\renewcommand{\noteA}{mW pr. fix at duty-cycle}
\renewcommand{\critB}{TTFF \& Availability}\renewcommand{\noteB}{Cold/warm/hot start}
\renewcommand{\critC}{RF-sensitivity \& antenna}\renewcommand{\noteC}{Patch-requirements, LNA}
\renewcommand{\critD}{Accuracy}\renewcommand{\noteD}{CEP50 typ.}
\renewcommand{\critE}{Size \& integration}\renewcommand{\noteE}{Footprint, layout}
\renewcommand{\critF}{Price \& Availability}\renewcommand{\noteF}{Unit price, lead-time}
\renewcommand{\critG}{Ecosystem \& tools}\renewcommand{\noteG}{u-center, AssistNow}

\renewcommand{\wA}{0.35}\renewcommand{\wB}{0.20}\renewcommand{\wC}{0.15}
\renewcommand{\wD}{0.10}\renewcommand{\wE}{0.10}\renewcommand{\wF}{0.05}\renewcommand{\wG}{0.05}

% Scores (1..5)
\renewcommand{\AoneA}{5}\renewcommand{\AoneB}{4}\renewcommand{\AoneC}{4}\renewcommand{\AoneD}{4}\renewcommand{\AoneE}{3}\renewcommand{\AoneF}{4}\renewcommand{\AoneG}{5}
\renewcommand{\AtwoA}{4}\renewcommand{\AtwoB}{4}\renewcommand{\AtwoC}{5}\renewcommand{\AtwoD}{4}\renewcommand{\AtwoE}{4}\renewcommand{\AtwoF}{4}\renewcommand{\AtwoG}{5}
\renewcommand{\AtriA}{2}\renewcommand{\AtriB}{3}\renewcommand{\AtriC}{3}\renewcommand{\AtriD}{3}\renewcommand{\AtriE}{4}\renewcommand{\AtriF}{4}\renewcommand{\AtriG}{3}

\DARsimple{Choise of positionsystem (GNSS)}
